MRE/Wave beta release General functions mrewave home data types reserved data input files output files clipboard resolution 1d plots 2d plots Wave inversion functions wave test data wave data wave parameters wave output wave unwrap wave filters wave lfe fftw faq known bugs |  |
Wave Inversion - filters
Six filters are available. Gaussian: LP: lowpass filter of order 'order'; passes frequencies lower than 'cutoff' BP: bandpass filter of order 'order'; passes frequencies between the lower and upper cutoffs. HP: highpass filter of order 'order'; passes frequencies higher than 'cutoff' Butterworth: LP: lowpass filter of order 'order'; passes frequencies lower than 'cutoff' BP: bandpass filter of order 'order'; passes frequencies between the lower and upper cutoffs. HP: highpass filter of order 'order'; passes frequencies higher than 'cutoff' Note: all 'cutoff' frequencies are specified in waves per FOV (field of view), referenced to the X-axis

MRE/Wave beta release For future updates check: http://mayoresearch.mayo.edu/mayo/research/ehman_lab"