MRE/Wave beta release General functions mrewave home data types reserved data input files output files clipboard resolution 1d plots 2d plots Wave inversion functions wave test data wave data wave parameters wave output wave unwrap wave filters wave lfe fftw faq known bugs |  |
getting started 1d plots
There are 3 ways in mrewave to open a 1d plot: 1: From the open window, select 1d when opening a file 2: Using the data desktop, after selecting a file, press . This will display the data with the chosen channel (in this case the i channel) 3: On the main toolbar pressing brings up the following window: This allows you to select lines, mix and match data from many sources, perform ft(s) and select basic plotting options. No matter how you bring up the plot, it's properties will be initialized from the following pages. 1d plot resolutions and functions Display properties of the plot can be modified with the lines and axis windows. When adding data to 1d plots, dimensions must be compatible. Data with different x dimensions can not be plotted together. Additionally each plane must have the same number of lines.

MRE/Wave beta release For future updates check: http://mayoresearch.mayo.edu/mayo/research/ehman_lab"