MRE/Wave beta release General functions mrewave home data types reserved data input files output files clipboard resolution 1d plots 2d plots Wave inversion functions wave test data wave data wave parameters wave output wave unwrap wave filters wave lfe fftw faq known bugs |  |
reserved data names
The following data names are reserved for mrewave. Data that contain [x,y] coordinate pairs, place the x coordinate is in the i channel and the y coordinate is in the q channel. These arrays can be displayed, edited, modified and deleted. Mrewave will overwrite or recreate them as needed. mrv_angle: complex i4[3,1,1,1] contains the x, y coordinates of the 3 points defining an angle. binary_copy: used for copy paste operations. Data type and size dependant on copy. mrv_profile: complex i4[2,1,1,1] contains the x, y coordinate of beginning and ending point of line. roi_mask: real n1. mask created by roi with 2D dimension compatible with currently selected data. roi_draw: complex i4[n,1,1,1] array of user drawn points defining a closed area. roi_ellip: complex i4[2,1,1,1] points define the extreme points of a rectangle that circumscribe an ellipse. roi_rect: complex i4[2,1,1,1] points define the extreme points of a rectangle. roi_fill: complex[1,1,1,1] value used to fill roi delete functions. Defaults to 0. roi_x: complex i4[2,1,1,1] points define a 1D roi containing the extreme x range. roi_y: complex i4[1,2,1,1] points define a 1D roi containing the extreme y range.roi_y: mrewave.filter: r4[] output of gaussian and butterworth filters.

MRE/Wave beta release For future updates check: http://mayoresearch.mayo.edu/mayo/research/ehman_lab"