MRE/Wave beta release General functions mrewave home data types reserved data input files output files clipboard resolution 1d plots 2d plots Wave inversion functions wave test data wave data wave parameters wave output wave unwrap wave filters wave lfe fftw faq known bugs |  |
faq
Q:How do I get data to Excel? A:The best way is to use the clipboard and save the data in text format. Q:How do I get images to Photoshop or PowerPoint? A:Save images as .bmp or .avi files. The clipboard can also be used to copy 8 and 24 bit bitmaps. Q:How do I get data to Matlab? A:You can exchange data between Matlab and mrewave through the use of Matlab .mat files. For slightly more information see output files. Q:Can mrewave write bitmaps, tif, jpeg....? A:mrewave can write bmp, gif, jpg, and png files. To save in a specific format just append the appropriate suffix. Q:What happens when a number larger than 32768 is saved to a pulsegen file or binary I2(16 bit integer) file? A:mrewave will flag this event. Large values will wrap around producing undesirable results.

MRE/Wave beta release For future updates check: http://mayoresearch.mayo.edu/mayo/research/ehman_lab"