MRE/Wave beta release General functions mrewave home data types reserved data input files output files clipboard resolution 1d plots 2d plots Wave inversion functions wave test data wave data wave parameters wave output wave unwrap wave filters wave lfe fftw faq known bugs |  |
Wave Inversion - mask
A mask can be applied to the phase image to facilitate phase unwrapping and wave inversion algorithms. mag threshold: The threshold value with which to create a mask from the input magnitude data. smooth: Checking this box smoothes the mask with a 9x9 median filter. limit regions: Check this box to restrict the number of connected regions in the mask. limit voids: Check this box to restrict the number of connected "voids" in the mask.

MRE/Wave beta release For future updates check: http://mayoresearch.mayo.edu/mayo/research/ehman_lab"